{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":4,"rows_kept":20,"merged":[[0,0,0,3],[20,0,23,3]],"flags":["formulas_cached_only"]}
["绿源污水处理监控系统清单"]
["设备、材料名称","型号","数量及单位","备注"]
["高清摄像头","1080P红外50米8mm3D降噪，移动侦测智能报警，数字宽动态。","4台"]
["录像机","8路nvr录像输入，支持多功能输入，多码流控制铁壳企业级录像机","1台"]
["硬盘","4T监控专用硬盘","1块"]
["监控杆地桩","普通","4根","3米"]
["网线","室外超五类无氧铜国标","2箱"]
["水晶头","RJ45镀金水晶头","1盒"]
["8口交换机","TP-link10/100/1000千兆","1台","9口百兆8口POE非网管PoE交换机"]
["16口交换机","TP-link10/100/1000千兆","1台","16口百兆非网管交换机"]
["套管","联塑阻燃管","300米"]
["摄像头支架","抱杆支架碳钢不锈钢紧轴","4个"]
["电源线","1.0国标","300米"]
["电源适配器","12V2A监控电源","4个"]
["插排","4~8孔","2个"]
["显示器","19寸","1台","19.5英寸LED背光宽屏液晶显示器"]
["室外配电箱","弱电箱","1个"]
["施工费"]
["发票",null,null,"含17%增值税票"]
["工程总造价"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}